**Destelheide** vzw Algemene Dienst voor Jeugdtoerisme Destelheidestraat 66, 1653 Dworp


Tel: +32 2 380 39 15 /Fax: +32 2 380 52 51

[info@destelheide.be](mailto:info@destelheide.be) /[www.destelheide.be](http://www.destelheide.be/)

# De Put hall technical sheet







|  |  |
| --- | --- |
| Hoofdgebouw – Algemeen grondplan | Main building – General floor plan |
| LADEN & LOSSEN | LOADING & UNLOADING |
| HOOFDINGANG | MAIN ENTRANCE |
| ONTHAAL | RECEPTION AREA |
| HAL | HALLWAY |
| Hoogspanning geen toegang | High voltage no access |
| Lokaal 011 opslagruimte / atelier | Room 011 storage space/workshop |
| Ingang loges (-1) | Entrance boxes (-1) |
| ZAAL “DE PUT” | “DE PUT” HALL |
| Uitschuifbare tribune 200 zitplaatsen | Extendable stand 200 seats |
| Ingang publiek | Entrance for the public |
| CAFETARIA | CAFETERIA |
| Glazen wand (met schuifdeur naar terras) verduisterbaar door geluiddempend gordijn. | Glass wall (with sliding door to the terrace) can be darkened by sound-absorbing curtain. |
| TERRAS | TERRACE |

General

* Entire room: 21 m x 21 m
* Height under the spot beams: 7 m
* Retractable grandstand with 200 seats can only be extended in full
* Capacity can be expanded to 350 seats with chairs
* Room can be darkened completely by electric window curtain; can only be operated from the balcony after explanation by the technician
* 1 curtain stage right and 1 curtain stage left; can be opened or closed by sliding
* Parquet floor
* 10-metre-wide x 8-metre-deep dance floor available
* 8 Hanging points and 4 water barrels available (see technical sheet ‘hanging points’)
* 32 podium elements 2 m² each (64 m²), adjustable height (20 cm to 80 cm)
* 2 pulpits
* Buffet piano (prices can be requested at the reception desk or from the technical team)
* 2 dressing rooms accessible from the De Put Hall, via a staircase

**each one contains**: 3 washbasins, 4 make-up mirrors with lamps, 2 dressing mirrors, 1 table, 10 chairs, 5 stools

***separately in the corridor****:* toilet, showers (2 for women, 2 for men)

* Catering: 15 walking dinner tables and 3 buffet tables (with canopy) available

Request (cross out what does not apply):

*Grandstand retracted/extended*

*Extra chairs (number: …)/no extra chairs  
Dance floor/no dance floor*

*Hanging points/no hanging points Water barrels/no water barrels*

*Podium elements (number: …)/no podium elements Pulpits/no pulpits*

*Buffet piano/no buffet piano   
Dressing rooms (number: …)/no dressing rooms*

*Walking dinner tables (number: …)/no walking dinner tables Buffet tables (number: …)/no buffet tables*

# Audio

* 6 speakers Active 2-Way Line-Array Module 2x8/1x2,5, 900W/RMS,
* 4 bass cabinets: Active 1x18" Subwoofer Bass-Reflex 1600W/RMS, RD-Net
* 7 speaker monitors JBL Eon610 active speakers
* 3 vocal microphones: SM58 (Shure)
* 4 wireless microphones (Sennheiser E835)
* 20 wired microphones: type Behringer and MICPRO1
* 8 stands for microphones (+ 20 table stands)
* Information about XLR cables and fittings can be obtained from the head technician.
* Small installation with mixing desk (brand: Allen&Heath ZED14) with max. 6 microphones (2 wireless and 4 with XLR connection or 6 with XLR connection),

2 CD players. Can be done without a technician.

* Mixing desk (brand: Behringer type: X32) controllable from the control room or from the hall. Destelheide technician always needed.

Audio request:

…

# Projector

* Projector type: Panasonic PT-DW830E
* Video projection on white electric extendible background screen (see below for size)
* Fixed projector with VGA and HDMI connection and wireless connection via Clickshare (will be explained on site)
* Mac adapter available for VGA and HDMI connection
* (Also available: overhead projector and small screen)

**Projector specifications: Panasonic PT-DW830E**

Number of pixels: 1,024,000 pixels (1280 x 800 dots)


Lens: electric zoom: 1.8 - 2.5:1 and electric focus: F = 1.7 – 1.9. f = 25.6mm – 35.7 mm Luminous lamp: 420 W UHM lamp x2


Light output: 8500 lumen (ANSI) Screen aspect ratio: 16:10

Request (cross out what does not apply):

*Use of projector and background screen/no use of projector and background screen  
Mac adapter/no Mac adapter*

*Overhead projector and small screen/no overhead projector and small screen*





|  |  |
| --- | --- |
| Zaal “De Put” – Inplanting projectiescherm + beamer | “De Put” Hall – Projection screen + projector installation |
| Jardin | Stage left |
| BALKON | BALCONY |
| Cour | Stage right |
| Projectiescherm 6.00m x 4.50m | Projection screen 6 m x 4.50 m |
| Tot wand | To wall |
| Beamer | Projector |
| Max. vrije hoogte | Max. free height |
| Vloer | Floor |


# Lighting

* 6x 2 KW **PC** spotlights
* 12x 1 KW **PC** spotlights
* 2x **profile** floodlights
* 20x 300 W **par** lamps
* 4 stands for individual spotlights available (which must be connected to the spot beams, no light connections on the sides or floor available)
* Complete colour book of colour filters
  + White (without filter)
  + Yellow (l100s)
  + Bright orange (l105r)
  + Pink (l113r)
  + Blue/green (l115r)
  + Dark blue (l118r)
  + Green (l121)
  + Dark green (l124)
  + Turquoise (l126r)
  + Dark blue (l141s)
  + Orange (l152r)
  + Red (164s)
  + Purple (l170s)
  + Blue (l174s)
* Mixing desk in the room: Lite-Puter CX-12, with 96 channels DMX dimming console, not programmable, operated manually.
* Mixing desk in the control room: ADB Cantor, with 96 channels, programmable, Destelheide technician always present. Can also be operated by a group technician upon presentation of a lighting technician's certificate.
* LED spots (100W/150W/160W/stage painters/stage beamers/cyclo bars/Moving heads/…) + Chamsys MagicQ MQ80


The backlight bar in the rear is a fixed light bar and can only be reached using an elevated work platform.  
Light bar 4 can only be reached via the grandstand with a ladder, not with an aerial platform.  
Side lighting via the balcony.

Lighting request: please make notes on the drawing on page 9


…



|  |  |
| --- | --- |
| Zaal “De Put” – Algemeen plafondplan | “De Put” Hall – General ceiling plan |
| Jardin | Stage left |
| BALKON | BALCONY |
| Cour | Stage right |
| Projectiescherm | Projection screen |
| Tegenlicht | Backlight |
| Lichtbalk | Light bar |
| Zijlicht jardin | Sidelight stage left |
| Zijlicht cour | Sidelight stage right |
| Ankerpunt | Anchor point |
| Beamer | Projector |
| Lichtspot (algemene verlichting) | Light spot (general lighting) |



|  |  |
| --- | --- |
| Zaal “De Put” – Inplanting lichtbalken | “De Put” Hall – Light bar installation |
| Jardin | Stage left |
| BALKON | BALCONY |
| Cour | Stage right |
| Tegenlicht | Backlight |
| Zijlicht jardin | Sidelight stage left |
| Zijlicht cour | Sidelight stage right |
| Lichtbalk | Light bar |
| Lichtbalken 1-2-3 | Light bars 1-2-3 |
| Max. vrije hoogte | Max. free height |
| Onderzijde balk | Bottom of bar |
| Zijlicht | Sidelight |
| Tegenlicht | Backlight |



|  |  |
| --- | --- |
| Zaal “De Put” – Aanvraag belichting / opmerkingen | “De Put” Hall – Request for lighting/ Comments |
| Jardin | Stage left |
| BALKON | BALCONY |
| Cour | Stage right |
| Projectiescherm | Projection screen |
| Tegenlicht | Backlight |
| Lichtbalk | Light bar |
| Zijlicht | Sidelight |
| ZAAL | HALL |
| Beamer | Projector |
| Op dit document kan je een schets maken van de gewenste belichting. Je kan hieronder ook nog opmerkingen kwijt: | On this document, you can draw a sketch of the desired lighting. You can also leave comments below: |

# Rules

* Loading and unloading is done via a sliding door where the unloading vehicle can be parked during loading and unloading only. Afterwards, it can be parked in the car park.
* Destelheide technicians are available during office hours, until 4 pm.
* Lighting, sound checks etc. must be requested in advance, both in terms of date and number of working hours.
* Technical assistance outside office hours will be charged.
* Ladders, aerial work platforms and light bars can be operated by your own qualified technician, provided that he/she takes responsibility in the event of damage and/or accident.
* Light bars are only suitable for hanging spotlights. No other weights or decor items can be hung from the bars. They cannot be used as a hoist.
* The balcony is only accessible to technicians.
* All materials you bring must comply with the applicable laws, Arab, Arei and Vlarem II.
* Technical materials can only be taken from backstage by a Destelheide technician.
* The use of smoke, fire, pyro-effects, water etc. is strictly prohibited.
* Smoking, eating and drinking are prohibited in the hall and on the stage.
* Damage to the parquet floor (for example, caused by decorative pieces) will be charged.
* If the group’s technician moves the spots, they must be returned to their original position afterwards (at the spot bars + plugged in).
* The room should be left swept and tidy after use.

Please send the completed technical sheet to reception at least two weeks in advance: info@destelheide.be

Technical assistance requested: yes/no *(cross out what doesn’t apply)*

If yes, on …………….. from ……………. until …………………

Set-up planned for …………….. from ……………. until …………………

Take-down planned for …………….. from ……………. until …………………